Last saved by: Spencer, Terre (CMDG-USA)

panel signage      10 14 23
1. Product Name
	Sign/Panel Support Systems
2. Manufacturer
Nova Display, Inc.
1626 Piner Road
Santa Rosa, CA  95403
Phone:	800-753-9688
Fax: 	800-753-0856
E-mail: 	enquiries@novadisplay.com
Website: 	www.novadisplay.com
3. Product Description
Nova Display offers practical, yet elegant sign/panel mounting systems with an infinite variety of display and signage mounting options. Easy to install, versatile and sturdy, these sign/panel support systems use quality hardware components that are available in a variety of finishes.
Basic Use
Nova Display sign/panel support systems are ideal for mounting indoor or outdoor display panels, architectural signs, directional and informational signage, company directories, and other decorative applications. Quality decorative hardware, unique designs and configurations effectively communicate the message, product or service.
Well-designed and precision engineered, the system components allow for flexible design configurations. Modular functionality and versatility ensure signage and displays can be easily designed and built as well as updated. The Nova Display sign/panel support system is:
	Easy to transport
	Re-configurable
	Simple assembly
	Variety of finishes
	Practical
	Lightweight
	Versatile
	Functional
	Easy to update
	Sleek
It allows various types of materials to be affixed to a wide range of substrates, including wood, gypsum, concrete, glass, aluminum profiles, steel studs, etc. Flexibility allows customization and synchronization of the sign/panel support system’s setting, color, material, finish and form to meet every requirement.
Components
Fittings are made of high-grade aluminum, brass or stainless steel for durability and consist of precision-machined components—standoffs, edge grips, projecting supports, grippers and screw caps—to provide an integrated solution to any signage and panel display requirements, while maintaining a consistent look throughout the installation. Parts are offered in a variety of quality finishes: clear anodized, satin chrome, polished chrome, brushed nickel and stainless steel. Supports of any shape, height or diameter can be combined to create the desired effect such as multi-layering or double-depth designs.
Applications
Nova Display’s sign/panel support systems offer a wide range of applications, including:

Frameless Graphic Panels
Special frames are designed to display posters, prints, photos or fine art reproductions enclosed between two pieces of acrylic or glass. The wall-mounted panels use panel standoff supports, allowing the display to be easily changed. The aesthetic appeal can be enhanced by varying the thickness, shape and type of panels used. Standard clear acrylic, as well as non-glare (non-reflective), color, frosted or textured acrylic, are available upon request.

Double-Depth Poster Display Panels
These acrylic poster frames provide a double-depth feature; the wall-attached base supports a clear, frosted or textured acrylic panel as a background screen. The front supports a graphic print or photo sandwiched between two clear acrylic panels, allowing the graphic to be easily changed. With a modern look, these double-depth poster display panels are ideal for art prints, posters or photography.
Butted Graphic-Display Panels
This graphic display consists of multiple panels butted closely together using one central fitting instead of four. Panels are mounted to walls using supports with special four-way connectors, allowing multiple posters or graphic prints to be displayed as a single large mural, graphic composition or backdrop. Supports can hold up to ^1⁄4 inch thick panels or two pressed pieces of ^1⁄8 inch thick acrylic with a poster or graphic print mounted in between the panels.
Logo Panels and Plaques
These high quality interior signage, plaques and logo panels are manufactured in various sizes, shapes, finishes and textures to afford a variety of uses.
Wall-Mounted Signage
These unique high-impact sign and award systems can be used in almost any environment by combining quality fittings and custom substrates.
Wall-Mounted Projecting Signage
These practical informational and directional wall-projected signs mount on projecting standoffs from the wall or ceiling. Message panels can be easily removed and replaced for maintenance or changing requirements.
Raised Glass Countertops
These custom countertops use safety glass or acrylic resin mounted on vertical standoff supports.
Architectural Paneling
This system provides mounted decorative or light-diffusing paneling on walls and/or ceilings.
Furniture Assembly
This solution can be used in contemporary furniture assembly.
Projecting Decorative and Product Shelving
This solution uses mounting glass and wooden shelves on walls or inside cabinets or showcases.
Composition and Materials
Brass Fittings
	C3604/CZ121 (CuZN39Pb3) brass
	Standard matte nickel/chrome plating finish
Note: 
Also available with polished chrome, polished brass and brushed (warm) nickel plating.
Aluminum Fittings
	High-grade aluminum
	Standard clear satin anodized plating finish
Note: 
Other custom finishes such as black or color anodized are available upon request.
Steel Fittings
	#SS201 or #SS304 stainless steel
	Standard brushed satin finish
Note: 
Custom finishes such as high-gloss polished are available upon request.
Grub Screws for Fitting
	Mild steel: 12L14
	Plastic Tip on grub screw: Nylon 66
Benefits
	Simplicity and practicality
	Easy to use
	Fully modular and customizable to specific needs
	
Re-configurable, allowing expedited and versatile updates of display materials
	
Extensive range of components and accessories ensure complete design flexibility and style
	
Durable and long-lasting products
Product Limitations
Use for indoor and outdoor with exception of brass fittings. Follow the instructions and weight-bearing limitation highlighted in technical data sheets available here.
Special Features
Frameless Poster Displays – Standard Kits
These frameless display panels are available in various sizes and configurations for use in artwork, poster and photo framing displays and presentations. Catalog information, technical specification and installations guides are available here.
Accessories
A number of accessories to enhance the utility and options of any sign/panel support system are available, including:
Easy Access Acrylic Pockets
These single or double sided pockets are designed to accommodate various sized posters, photos, graphic art and documents.  Available to suit any display requirement and customizable to meet any design variations.
Hook-on Acrylic Pockets
An alternative to traditional slat-wall systems, these pockets are designed to hook on horizontal rods, mounted on wall or suspended on cables. Easy to install; help create stylish interior displays for any type of information, but can be readily changed in minutes. All pockets hook onto rods without using any tools. Used on walls or windows in estate and recruitment agencies, offices, receptions, museums, etc.
Wall-Mounted Poster Frames
These frameless graphic panels are designed for displaying posters, prints, photos or fine art reproductions by pressing them between two pieces of acrylic or glass. The thickness, shape and type of panels may vary depending on the desired effect. The panels are mounted to walls using panel supports (wall spacers). Available in standard clear acrylic back panel with a non-glare (non-reflective) front, or with color, frosted, printed backing, etc.
Acrylic Leaflet Dispensers
These prefabricated and custom fabricated leaflet dispensers come in many unique styles and sizes. Dispensers  are manufactured from exceptional quality, clear, lightweight acrylic. Options include cable suspended, hooked-on horizontal rod, wall mounted on spacers, single, or multi-pocket leaflets versions. Available in standard design or customized version upon request.
Cable/Rod Suspended Showcase Displays
These displays are available with a locking mechanism for maximum security, or with an open front and back so that the reflection of the acrylic does not affect the displayed items. Each unit can be supplied with low voltage lights suspended from the cables, with the light beam directed through the open holes for maximum lighting effect. Custom built cases are available upon request.
Stock Glass and Acrylic Shelving
Standard clear tempered glass and acrylic shelving are available in most popular sizes and edge finishes at competitive prices. These glass and acrylic shelves are primarily used for cable/rod suspended shelving, product display cases, furniture, etc.
View all display kits and concept ideas from Nova Display here.
Custom Services
Nova Display Systems has the capability and expertise to take any ideas or concept and then craft them into functional, well designed and environmentally friendly display products. Contemporary showcases, unique signs, or a sophisticated donor recognition wall display are a few of the applications possible. View more Nova Display custom services here.
This capability to fabricate extends beyond the use of acrylics, glass, or modular aluminum profiles. Custom fabrication on a much smaller scale is also available for designing and fabricating individual metal components and fittings using aluminum, brass and copper alloys, stainless steel, etc. 
Nova Display Systems provides personalized support and exceptional quality of fabrication. For customized display or sign products, client can send specifications and sketches using the downloadable quote form here.
4. Technical Data
Applicable Standards
American Iron and Steel Institute (AISI)
	
AISI 12L14 Carbon Steel (UNS G12144)
American National Standards Institute (ANSI)
	
AL 6063/6063A Properties, Fabrication and Applications, Extruded Aluminum Alloy
American Society for Testing and Materials (ASTM)
	
ASTM B16 Standard Specification for Free-Cutting Brass Rod, Bar and Shapes for Use in Screw Machines (UNS C3600/3604)
	
ASTM B124 Standard Specification for Copper and Copper Alloy Forging Rod, Bar and Shapes (UNS C37710)

Unified Numbering System (UNS) (alloy designation system)
	UNS C3600/3604 free-cutting brass
	UNS C37710 leaded brass/forging brass
	UNS G12144 carbon steel
Sustainment
Nova Display Systems’ minimalist design simplifies and purifies the content to reveal the essential quality and functionality of the product; removing clutter with the minimal usage of materials.
All display systems are fabricated from non-ferrous recycling metals such as aluminum, stainless steel, brass, bronze and copper alloys. With close to 100 percent recyclable content, these metals can be repeatedly recycled back into similar or other products with no loss of quality, as reprocessing does not damage their molecular structure.
Fire Performance
Sign/panel support fittings are produced from aluminum, which has a melting point of over 1220 Degrees F, 660 C), brass CZ121, which has a melting point of over 1652 degrees F, (900 C) and stainless steel Grade 201 or 303, which has a melting point of 2552—2642 degrees F, (1400–1450 C); the plating materials of nickel and chromium have melting points of over 2552 degrees F, (1400 C), so none are considered a fire hazard.
Weight-Bearing Limitations
Recommended load-bearing per standoff diameter and material  (per one fixing mounted on drywall):
Aluminum Supports/Wall Mounted Options:
	15 mm (^5⁄8 inch) diameter: 8 pounds (3.5 kgs)
	20 mm (^3⁄4 inch) diameter: 15 pounds (6.8 kgs)
	25 mm (1 inch) diameter: 25 pounds (11 kgs)
Brass Supports/Wall Mounted Options:
	12 mm (^1⁄2 inch) diameter: 5 pounds (2 kgs)
	15 mm (^5⁄8 inch) diameter: 8 pounds (3.5 kgs)
	20 mm (^3⁄4 inch) diameter: 15 pounds (6.8 kgs)
	25 mm (1 inch) diameter: 25 pounds (11 kgs)
Stainless Steel Supports/Wall Mounted Options:
	12 mm (^1⁄2 inch) diameter: 5 pounds (2 kgs)
	15 mm (^5⁄8 inch) diameter: 8 pounds (3.5 kgs)
	20 mm (^3⁄4 inch) diameter: 15 pounds (6.8 kgs)
	25 mm (1 inch) diameter: 25 pounds (11 kgs)
	30 mm (1^3⁄16 inch) diameter: 25 pounds (11 kgs)
5. Installation Instructions
Preparatory
Additional blocking in the wall may be required for mounting heavier panels. For specific product installation instructions click here.
Methods
For parts specifications such as sizes, stud and screw threads, panel hole diameter, panel thickness, mounting screw size, etc., click here.
Important: 
Consult the appropriate installation guide for any of the items listed here:
	
Aluminum stand-offs
	Wall-mounted supports for signs
	Wall support system
	Through standoff supports and spacers
	Edge-grip and projecting supports
	Graphic holders
	Poster frames
	Display tracks and anchors
	Cable/rod suspended poster displays
	Wall-mounted poster displays
Precautions (Performance, Safety)
Always check the installation surface to ensure the substrate is strong enough to hold the weight of the panel. All installation must be done so with proper hardware and protective gear to ensure safety.
Weather/Ambient Considerations
	
Brass and #SS201 stainless steel components are suggested for interior use only
	
Aluminum and #SS304 stainless steel components can be used for indoor and outdoor
	
For high-humidity and other special environments request #SS316 stainless steel items that can be made to order

Delivery, Storage and Handling
Most components are small and do not require any special packaging or handling.
6. Availability and Cost
Availability
Most of the standard components are stocked and delivered in 2–15 business days. Lead time on non-standard items, special item or customized product may vary from up to 10–12 weeks.
Cost
Pricing and specifications for most products can be found here.
All prices are quoted in U.S. dollars. The listed prices are FOB Santa Rosa, California USA and do not include freight charges or any applicable taxes. All prices are subject to change without notice.
No deduction is allowed at settlement. Prices for certain government, corporate and institutional customers may be set forth in a bid or other written agreement between the parties.
If unsure what components need to be ordered, please fax or email Nova Display a short description or graphical attachment (i.e., a rough sketch or project layout).
7. Warranty
Nova Display Systems, Inc., manufactures hardware products from parts and components that are new or equivalent to new in accordance with industry-standard practices. Nova Display warrants that the hardware products it manufactures will be free from defects in materials and workmanship. The warranty term is one year beginning on the date of purchasing, or the date the merchandise is received by the customer.
This warranty does not cover damage due to external causes, including accident, abuse, misuse, failure to follow installation requirements and problems caused by use of parts and components not supplied by Nova Display. Any unauthorized opening of the merchandise enclosure(s) will void this warranty in its entirety as it pertains to that item.
Nova Display will replace products returned to Nova Display facility. To request warranty service, contact Nova Display within the warranty period. If warranty service is required, Nova Display will issue a Return Merchandise Authorization Number (RMA number). Ship the products back to Nova Display in their original or equivalent packaging, prepay shipping charges and insure the shipment or accept the risk of loss or damage during shipment. 
Nova Display will ship the repaired or replacement products back, freight prepaid, if the address is in the U.S. Shipments to other locations will be made freight collect. Nova Display may, but is not required to, ship replacement components prior to receiving the returned merchandise. If so and if the return merchandise is not received in good condition (less the repair issue for which the RMA was issued) the customer will be responsible for paying the full list price of the merchandise that was sent as a replacement.
Nova Display owns all replaced parts. Nova Display uses new and reconditioned parts made by various manufacturers in performing warranty repairs and building replacement products. If Nova Display repairs or replaces a product, its warranty term is not extended.
This warranty gives customers specific legal rights and they may also have other rights, which vary from state to state (or jurisdiction to jurisdiction). Nova Display’s responsibility for malfunctions and defects in hardware is limited to repair and replacement as set forth in this warranty statement. Suitability and fitness for a particular purpose are expressly disclaimed.
All express and implied warranties for the product, including but not limited to any implied warranties of and conditions of merchantability, are limited in duration to the warranty period set forth above and no warranties, whether express or implied, will apply after such period. Some states (or jurisdictions) do not. Allow limitations on how long an implied warranty lasts, so the above limitation may not apply.
A downloadable .pdf file of warranty policies is here.
8. Maintenance Instructions
Does not require servicing. Download installation instructions here.
Inspect cables and fittings regularly for visible damage, wear, elongation, kinking, crushing, corrosion, etc. No product can keep operating at its rated capacity indefinitely. Periodic inspections help determine when to replace a cable to eliminate extensive damage or reduce hazards.
9. Technical Services
Design Services/Creative Design and Project Development
Nova Display Systems, Inc., specializes in design, planning and project management. It assists in specifying any part of the project and helps develop the client’s idea from prototype to production.
Nova Display works with a highly specialized team of interior designers, decorators, contractors and other service providers who have the training and expertise to manage all project details. 
Contact Nova Display’s in-house design team or request information about its Preferred Design Partner Program of certified architects and design companies nearby.
For more information, please contact Nova Display’s main office or click here.
Installation Services
For installation assistance, click Installation Instructions for most Nova Display systems or individual components. Installation services are also available through Nova Display’s Preferred Installer Program of certified contractors located nearby. Contact Nova Display Systems, Inc., for any questions not available through these resources.
10. Filing Systems
	CMD

Additional product information is available from Nova Display Systems, Inc., upon request